{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["戴俊城涡轮（39）","戴俊城质量流量计（42）"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"戴俊城涡轮（39）","index":0,"n_rows":49,"n_cols":12,"rows_kept":49,"merged":[[0,0,2,1],[0,2,1,3],[0,4,0,5],[0,6,0,10],[1,4,1,5],[1,6,1,10],[2,2,2,3],[2,4,2,5],[2,6,2,10],[3,0,3,1],[3,6,3,10],[4,0,4,2],[4,3,4,5],[4,6,4,8],[4,9,4,10],[5,0,6,2],[5,3,5,5],[5,6,5,8],[5,9,5,10],[6,3,6,5],[6,6,6,8],[6,9,6,10],[7,0,7,2],[7,3,7,5],[7,6,7,8],[7,9,7,10],[8,0,8,2],[8,3,8,5],[8,6,8,8],[8,9,8,10],[9,0,17,0],[9,1,9,2],[9,3,9,5],[9,6,9,8],[9,9,9,10],[10,1,10,2],[10,3,10,5],[10,6,10,8],[10,9,10,10],[11,1,11,2],[11,3,11,5],[11,6,11,8],[11,9,11,10],[12,1,12,2],[12,3,12,5],[12,6,12,8],[12,9,12,10],[13,1,13,2],[13,3,13,5],[13,6,13,8],[13,9,13,10],[14,1,14,2],[14,3,14,5],[14,6,14,8],[14,9,14,10],[15,1,15,2],[15,3,15,5],[15,6,15,8],[15,9,15,10],[16,1,16,2],[16,3,16,5],[16,6,16,8],[16,9,16,10],[17,1,17,2],[17,3,17,5],[17,6,17,8],[17,9,17,10],[18,0,26,0],[18,1,18,2],[18,3,18,5],[18,6,18,8],[18,9,18,10],[19,1,19,2],[19,3,19,5],[19,6,19,8],[19,9,19,10],[20,1,20,2],[20,3,20,5],[20,6,20,8],[20,9,20,10],[21,1,21,2],[21,3,21,5],[21,6,21,8],[21,9,21,10],[22,1,22,2],[22,3,22,5],[22,6,22,8],[22,9,22,10],[23,1,23,2],[23,3,23,5],[23,6,23,8],[23,9,23,10],[24,1,24,2],[24,3,24,5],[24,6,24,8],[24,9,24,10],[25,1,25,2],[25,3,25,5],[25,6,25,8],[25,9,25,10],[26,1,26,2],[26,3,26,5],[26,6,26,8],[26,9,26,10],[27,0,37,0],[27,1,27,2],[27,3,27,5],[27,6,27,8],[27,9,27,10],[28,1,28,2],[28,3,28,5],[28,6,28,8],[28,9,28,10],[29,1,29,2],[29,3,29,5],[29,6,29,8],[29,9,29,10],[30,1,30,2],[30,3,30,5],[30,6,30,8],[30,9,30,10],[31,1,31,2],[31,3,31,5],[31,6,31,8],[31,9,31,10],[32,1,32,2],[32,3,32,5],[32,6,32,8],[32,9,32,10],[33,1,33,2],[33,3,33,5],[33,6,33,8],[33,9,33,10],[34,1,34,2],[34,3,34,5],[34,6,34,8],[34,9,34,10],[35,1,35,2],[35,3,35,5],[35,6,35,8],[35,9,35,10],[36,1,36,2],[36,3,36,5],[36,6,36,8],[36,9,36,10],[37,1,37,2],[37,3,37,5],[37,6,37,8],[37,9,37,10],[38,0,38,2],[38,3,38,5],[38,6,38,8],[38,9,38,10],[39,0,39,2],[39,3,39,5],[39,6,39,8],[39,9,39,10],[40,0,40,2],[40,3,40,5],[40,6,40,8],[40,9,40,10],[41,0,41,2],[41,3,41,5],[41,6,41,8],[41,9,41,10],[42,0,44,10],[45,2,45,3],[45,5,45,6],[45,7,45,8],[46,2,46,3],[46,5,46,6],[46,7,46,8],[47,2,47,3],[47,5,47,6],[47,7,47,8],[48,2,48,3],[48,5,48,6],[48,7,48,8]],"flags":["formulas_cached_only"]}
["浙江衢化氟化学有限公司",null,"仪表数据表",null,"工程名称"]
[{"$nulls":4},"设计项目"]
[null,null,"电磁流量计",null,"图号"]
["用户",null,"合同号",null,"设计阶段","施工图","第     页         共    页"]
["位号 "]
["用途"]
[]
["P＆ID号"]
["设备位号"]
["操作条件","工艺介质",null,"天然气"]
[null,"操作压力Mpa(G)",null,"2.5MPa"]
[null,"操作温度℃",null,"，-30℃～80℃"]
[null,"最大流量","最大流量",{"$nulls":8},"1、仪表采用进口专用精密轴承，摩擦阻力小，密封性好。"]
[null,"正常流量","正常流量","700N/m3",{"$nulls":7},"2、涡轮叶片抗磁干扰，增加检测精度，保证检测的可靠性。"]
[null,"最小流量","最小流量",{"$nulls":8},"3、流量积算仪可350°旋转，安装方便。"]
[null,"操作状态粘度MPa.s","操作状态粘度MPa.s",{"$nulls":8},"4、控制信号输出，可设置上下限报警"]
[null,"操作状态密度kg/m3","操作状态密度kg/m3",{"$nulls":8},"5、修正仪有自检功能，方便用户检修和调试。"]
[null,"分子量","形式",{"$nulls":8},"6、内置加油系统，实现一体化润滑。"]
["传感器规格","型号","型号"]
[null,"供电方式",null,"24VDC/3.6V 锂电池供电"]
[null,"测量范围","测量范围"]
[null,"公称直径( mm)","公称直径( mm)"]
[null,"本体材质","本体材质","316L"]
[null,"衬里材质","衬里材质"]
[null,"内件材质","电极材质","316L"]
[null,"法兰标准及尺寸","法兰标准及等级","HG/T20592 SO125（B）-16 RF"]
[null,"过滤器"]
["变送器规格","型号","型号"]
[null,"输出信号","输出信号","4-20MA（两线制）三线制脉冲频率信号+hart "]
[null,"精度","精度",1.5]
[null,"电源","电源"]
[null,"电气接口","电气接口","1/2NPT"]
[null,"防爆等级","防爆等级","ExdIICT6"]
[null,"防护等级","防护等级","IP68"]
[null,"积算"]
[null,"电气接口尺寸","法兰尺寸及密封面"]
[null,"安装形式","安装形式"]
[null,"附件","附件"]
["量程比",null,null,"01:30:00"]
[]
[{"$nulls":3},"带TS管道认证证书"]
["制造厂"]
[]
[]
[]
[]
[]
[]
["版次","说   明","设  计",null,"日  期","校  核",null,"日  期",null,"审 核","日  期"]

{"sheet":"戴俊城质量流量计（42）","index":1,"n_rows":32,"n_cols":4,"rows_kept":32,"merged":[[0,0,1,1],[0,3,0,4],[1,3,1,4],[2,0,2,1],[2,3,2,4],[3,0,3,1],[4,0,4,1],[5,0,5,1],[6,0,6,1],[7,0,11,0],[12,0,28,0],[12,3,12,4],[21,4,22,4]],"flags":["formulas_cached_only"]}
["浙江衢化氟化学  有限公司",null,"工程名称","自动化仪表整改"]
[null,null,"设计项目"]
["单直管质量流量计",null,"图号"]
["位号 ",null,"数量：3台"]
["用途"]
["P＆ID号"]
["管道编号/设备位号"]
["操作条件","工艺介质","氟硅酸，盐酸"]
[null,"操作压力MPaG","常压"]
[null,"操作温度℃","常温"]
[null,"操作密度kg/m3","500-2500"]
[null,"操作流量(T/h)",15]
["仪表规格","型号","单直管质量流量计","（希望售后服务可以跟上，现场安装可以进行视屏通话指导）"]
[null,"传感器形式"]
[null,"测量范围(T/h)",15]
[null,"精度","±0.2%"]
[null,"输出信号","4-20mA+485"]
[null,"电源","24VDC"]
[null,"电气接口尺寸","1/2”NPT"]
[null,"元件材料","HC+衬PFA"]
[null,"杆子长度"]
[null,"测量管内径（mm）","≥35"]
[]
[]
[]
[null,"防爆等级","ExdⅡBT4"]
[null,"防护等级","IP65"]
[null,"工艺连接尺寸","HG/T 20592 SO50(B)-16  RF"]
[null,"法兰材质"]
[]
[]
["制造厂"]