{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["需定铂电阻"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"需定铂电阻","index":0,"n_rows":12,"n_cols":14,"rows_kept":12,"merged":[[0,0,0,13],[11,0,11,12],[12,0,12,12]],"flags":["formulas_cached_only"]}
["锦华公司JH-6项目铂电阻清单"]
["序号","仪表位号","仪表名称","型号","L×l","保护管形式","保护管直径","保护管及法兰材质","接口规格","介质温度℃","介质表压力MPa","数量（支）","备注","厂家"]
[3,"TE-2502","法兰焊接式整体钻孔铂热电阻","WZP-440F","550×400","整体钻孔套管","∅25/∅16×∅9（尾部）","316L+PFA","法兰HG20592 SO40（B）-16 RF ",60,0,1,"保护管整体钻孔后，压铸PFA。","巨化仪表"]
[4,"TE-2504A，2504B，2504C，2504D，2504E","法兰焊接式整体钻孔铂热电阻","WZP-440F","600×450","整体钻孔套管","PFA衬后外径20mm。","316L+PFA","法兰HG20592 SO25（B）-16 RF ",85,-0.065,5,"保护管整体钻孔后，铸塑PFA。","巨化仪表"]
[5,"TE-2511B，2511C","法兰焊接式整体钻孔铂热电阻","WZP-440F","550×400","整体钻孔套管","PFA衬后外径20mm。","316L+PFA","法兰HG20592 SO25（B）-16 RF ",85,-0.065,2,"保护管整体钻孔后，铸塑PFA。","巨化仪表"]
[9,"TE-2511A","法兰焊接式整体钻孔铂热电阻","WZP-440F","500×350","整体钻孔套管","PFA衬后外径20mm。","316L+PFA","法兰HG20592 SO25（B）-16 RF ",75,-0.065,1,"保护管整体钻孔后，铸塑PFA。","巨化仪表"]
[12,"TE-2544，2612，2717，2720","法兰焊接式整体钻孔铂热电阻","WZP-440F","550×400","整体钻孔套管","PFA衬后外径20mm。","316L+PFA","法兰HG20592 SO25（B）-16 RF ",85,-0.07,4,"保护管整体钻孔后，铸塑PFA。","巨化仪表"]
[13,"TE-2513A，2513B，2532，2610，2611，2715，2716，2718，2719","法兰焊接式整体钻孔铂热电阻","WZP-440F","600×450","整体钻孔套管","PFA衬后外径20mm。","316L+PFA","法兰HG20592 SO25（B）-16 RF ",85,-0.07,9,"保护管整体钻孔后，铸塑PFA。","巨化仪表"]
[18,"TE-2602，2603，2604，2605，2606，2702，2703，2704，2705，2706，2707，2708，2709，2710，2711","法兰焊接式整体钻孔铂热电阻","WZP-440F","600×450","整体钻孔套管","PFA衬后外径20mm。","316L+PFA","法兰HG20592 SO25（B）-16 RF ",85,-0.065,15,"保护管整体钻孔后，铸塑PFA。","巨化仪表"]
[21,"TE-2701","法兰焊接式整体钻孔铂热电阻","WZP-440F","600×450","整体钻孔套管","PFA衬后外径20mm。","316L+PFA","法兰HG20592 SO25（B）-16 RF ",80,0.006,1,"保护管整体钻孔后，铸塑PFA。","巨化仪表"]
[null,"合计",{"$nulls":9},38]
["说明：1、以上所有温度计的防爆等级全为ExdⅡBT4；   2、电气接口为：M20×1.5。 加急 货期10.20"]